**BMP L611 – Concentrated Flow Dispersion Sizing Sheet for Minimum Requirement #5 – The List Approach**

# Concentrated flow dispersion BMPs shall be designed in accordance with the SWMM and Green Stormwater Infrastructure Typical Detail Figure 009 – Concentrated Flow Driveway Dispersion. Clearly show the vegetated flowpath on the site plan. A maximum of 700 ft2 of roof area can drain to each dispersion BMP.

# Hard Surface Area Requiring Mitigation: Click here to enter text.

# Hard Surface Draining to Dispersion BMP: Click here to enter text.